{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":10,"n_cols":21,"rows_kept":10,"merged":[[1,0,1,20],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,2,7],[2,8,3,8],[2,9,2,10],[2,11,3,11],[2,12,2,16],[2,17,2,19],[2,20,3,20]],"flags":["formulas_cached_only"]}
["附件"]
["石城县2022年国家水土保持重点建设工程及小型农田水利建设项目计划批复表"]
["序号","项目类别","项目名称","建设性质(新建/续建)","时间进度\n(建设起止年月)","实施地点",null,null,"建设任务（内容）","资金规模和筹资方式",null,"资金来源","绩效目标",{"$nulls":4},"责任单位",null,null,"备注"]
[{"$nulls":5},"乡（镇）","村","是否重点帮扶村",null,"总投资(万元)","其中：整合财政涉农资金",null,"效益指标（带农联农效果）","产出指标\n（项目产出成果）","受益\n户数\n（户）","受益\n人口数\n（人）","满意度指标(≥%)","项目主管单位","项目实施单位","后续管护单位"]
["总计",{"$nulls":8},615,615]
[1,"基础设施","石城县2022年国家水土保持重点工程新龙河小流域综合治理项目","新建","2022年1月—2022年12月","龙岗乡","新龙村、绿水村、龙岗村、水庙村等","是","1、工程措施;整治河道约1km，新建格宾挡墙护岸约1.7km，排灌沟渠（40×40cm）1km，排灌沟渠（50×60cm）0.5km。2、林草措施：整治边坡800㎡。3、水保林21.75h㎡。4、封禁管护1195.69h㎡",430.7,430.7,"中央水利发展资金、省级水利专项资金","各项水土保持措施产生的总经济效益为4157.98万元，单位治理面积年均直接经济效益为328.95万元。小流域内每年可增加保土3.79万t，增加蓄水能力120.20万m3，减沙效率达到70.0%以上，受益户900户。","整治河道约1km，建成格宾挡墙护岸约1.7km，排灌沟渠（40×40cm）1km，排灌沟渠（50×60cm）0.5km。2、林草措施：整治边坡800㎡。3、水保林21.75h㎡。4、封禁管护1195.69h㎡",900,4500,95,"县水利局","县水土保持中心","有关村"]
[2,"基础设施","石城县2022年国家水土保持重点工程福田小流域综合治理项目","新建","2022年1月—2022年12月","丰山乡","福村村、懒田村、下坑村、大琴村、陈江村等","部分","1、工程措施;新建格宾挡墙（高度4.5m，顶宽1.0m）150米，新建挡墙浆砌石挡土墙（高度4.5m，顶宽1.0m）15米，2、封禁管护283h㎡",50.8,50.8,"中央水利发展资金、省级水利专项资金","各项水土保持措施产生的总经济效益为815.79万元，单位治理面积年均直接经济效益为76.60万元。小流域每年可增加保土3.25万t，增加蓄水能力102.14万m3，减沙效率达到70.0%以上，受益户2240户。","建成格宾挡墙（高度4.5m，顶宽1.0m）150米，浆砌石挡土墙（高度4.5m，顶宽1.0m）15米，2、封禁管护283h㎡",2240,11200,95,"县水利局","县水土保持中心","有关村"]
[3,"基础设施","杨天坑山塘维修加固","新建","2022年1月—2022年12月","小松镇","蜀口村","是","上游粘土斜墙900m³，下游坝体整坡550m³，破坝拆除重建坝下涵管60m，拆除重建放水斜管及消力水箱25m³，混凝土溢洪道加固78m³等。",59,59,"中央水利发展资金、省级水利专项资金","保障人民生命财产安全，保障农业生产灌溉用水，受益户120户。","建成上游粘土斜墙900m³，下游坝体整坡550m³，破坝拆除重建坝下涵管60m，拆除重建放水斜管及消力水箱25m³，混凝土溢洪道加固78m³等。",120,600,95,"县水利局","县水土保持中心","蜀口村"]
[4,"基础设施","麻窝山塘维修加固","新建","2022年1月—2022年12月","大由乡","王沙村","是","上游坝体培厚320m³，下游坝体整坡380㎡，拆除重建放水斜管及消力水箱16m³，混凝土溢洪道加固27m³等。",19,19,"中央水利发展资金、省级水利专项资金","保障人民生命财产安全，保障农业生产灌溉用水，受益户170户。","上游坝体培厚320m³，下游坝体整坡380㎡，拆除重建放水斜管及消力水箱16m³，混凝土溢洪道加固27m³等。",170,520,95,"县水利局","县水土保持中心","王沙村"]
[5,"基础设施","谢古坑山塘维修加固","新建","2022年1月—2022年12月","琴江镇","长天村","是","上游坝体培厚685m³，下游坝体整坡750㎡，新建坝下涵管76、放水斜管及消力水箱32m³，混凝土溢洪道加固68m³等。",55.5,55.5,"中央水利发展资金、省级水利专项资金","保障人民生命财产安全，保障农业生产灌溉用水，受益户50户。","上游坝体培厚685m³，下游坝体整坡750㎡，新建坝下涵管76、放水斜管及消力水箱32m³，混凝土溢洪道加固68m³等。",50,200,95,"县水利局","县水土保持中心","长天村"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}